# Feature of product

OLED large screen, rich interface.

Precise position of data scale.

Layering display backfat thickness.

Data storage and transfer function.

# Product details introduction

Technical Specifications

|  |  |
| --- | --- |
| Measuring Range | 4~45mm |
| Battery Capacity | Li 3.7V 1200mah |
| Charging Input Voltage | Dc 5V Micro Usb |
| Monitor | Oled 1.3 Inch |
| Data Storage | 999 |
| Operating Environment Temperature | 0~40 ℃ |
| Application Range | Swine |

Standard Configuration

**Main unit/Probe/Battery/Adapter/USB cable/couplant/User’s manual**